Teamcenter Integration Refile Utility

   -u[ser]=<user> : To specify Teamcenter user name

   -g[roup]=<group> : To specify Teamcenter group name

   -p[assword]: To specify Teamcenter password

   -pf=<filename> : File to specify the Teamcenter password

   -i[nput_list]=<filename> : List of specifications of parts to refile. 
   Part name should be in the @DB/<Item ID or Part Identifier>/<rev_id> format, 
   where Part Identifier is fnd0partIdentifier property on Item

   -f[older]=<foldername> : Name of folder listing parts to refile

   -k[eep_volume]=<yes|no> : Use original volume for refiled parts. Default <yes>

   -h[elp]: Produces this message

   -d[rawings]=<update> : Update drawings

   -non[_masters]=<yes|no> : Automatically refile non-master parts.Default <yes>

   -out[put_file]=<filename> : File to write failure information to

   -log[_file]=<filename> : File to write log information to

   -part=<part spec> : Specification of single part to refile.
   Part name should be in the @DB/<Item ID or Part Identifier>/<rev_id> format, 
   where Part Identifier is fnd0partIdentifier property on Item

   -bypass=<yes|no> : Use bypass privilege if necessary. Default <yes>

   -resume[_from]=line number of input list to start processing from

   -update_mod[_props]=<yes|no> : Update last modifying user/date on dataset

   -set_new_dataset_o[wner]: Sets the ownership of new datasets to be either that 
   of the owning item-rev or multi-CAD jt dataset

   -refile_released=<yes|no> : Refile parts with release status. Default <no>

   -structure_sync=<no|from_teamcenter|from_ug> : Synchronize structures during refile. Default <no>

   -force_structure_sync=<yes|no> : Force synchronize structures during refile 
   as requested by -structure_sync. Default <no>

   -transforms_source=<from_teamcenter|from_ug> : Source of transforms if different 
   from -structure_sync argument. Default <from_ug>

   -allow_null_transform used with -structure_sync=from_teamcenter 
   and -transforms_source=from_teamcenter to allow transforms 
   from Teamcenter to be null

   -sync_arrangements=<yes|no> : Synchronize arrangement data if consistent with 
   other structure sync settings. Default <no>

   -read_mapped_attri[butes]=<yes|no> : Read mapped attributes if consistent with 
   other structure sync settings. Default <yes>

   -generate_trueshape=<yes|no> : Generate True Shape occupancy data without 
   refiling parts. Default <no>

   -record_part_data=<yes|no> : Record part data (Bounding Box, Mass Properties) 
   without refiling parts. Default <no>

   -record_altrep_notes=<yes|no> : Record AltRep occurrence notes without refiling 
   parts. Default <no>

   -compression=<compress|uncompress> : Compresses|uncompresses the part(s) 
   when refiling

   -y: Fully load assembly and refile components that are not at the current 
   version of NX

   -force_refile: Used with the -y switch to force all components to be refiled

   -cleanu[p]=<yes|no> : Perform part cleanup before refiling. Default <no>

   -anon[ymize]=<yes|no> : Removes user and program version strings from part 
   history. Default <no>

   -force_read_jt: Force to read from a JT dataset even if a master dataset exists

   -convert_mcs=<filename> : Convert mating conditions to assembly constraints and 
   output report

   -mc_parts_only: Used in conjunction with convert_mcs to specify only convert 
   parts which contain mating conditions

   -mc_dry_run: Used in conjunction with convert_mcs to do the mating condition 
   conversion and generate the conversion report without saving any parts.

   -mc_dont_load_referenced_geometry: Used in conjunction with convert_mcs to 
   not load geometry referenced by the mating conditions being converted. 
   Note this will bypass constraint conversion checking.

   -regen_lw: Force all lightweight bodies in the specified part to be regenerated.
   By default the faceting parameters previously used to create each body will be       
   used again. This option is now being done by default for parts saved 
   before NX7.5.

   -regen_lw_def_tol: Similar to regen_lw however this flag will not use the 
   faceting parameters on the existing body but the default faceting parameters       
   will be utilized instead.

   -remap_drawing_callouts=<attribute_name> : Remap the callout references in 
   drawing to <attribute_name>

   -synchronize_callout_to_teamcenter=<normal|force_skip_one_level> :
   Update the Find No. in Teamcenter based on the CALLOUT value on the NX part occurrences

   -convert_units_to_mm: Convert the refiled part from inches to millimeters

   -convert_units_to_in: Convert the refiled part from millimeters to inches

   -recreate[_missing_stock_components]: For Routing assemblies, re-creates any missing stock as component components

   -convert_line_widths: Converts all legacy line width in the specified parts to use new line widths. 
   Conversion is done based on the Legacy Line Width Conversion part preference.

   -create_drawing_snapshot: Creates snapshot data of the part for its drawings

   -use_default_load_option_file: Uses specified default load options.
   This cannot be used along with -y option, -y option takes precedence if set

   -refile_specified_non_master_only: Used with -input_list option to refile 
   Only specified non-master while processing the non-master parts form the input list

